CDS Version 1.04





Version 1.04 Release July 2000





This is a further incremental release which rectify’s more bugs that have been reported in the last year. This version is still supported and we will continue to release additional bug fix’s when necessary.





Some of the more notable fixes are listed below.





“Killing Jobs” – three of you somehow managed to be able to kill a job by somehow having two copies of the job, with the same name, but living in different locations, and having them both open at the same time. We believe that we have removed the possibility of this happening again, although, we never cease to be amazed by the ingenuity of our clients when it comes to placing your hard earned data in danger.


As a side bar to this problem, it is NOT a backup if it is living on the same computer and open at the same time as the original copy !!!





Import – we have considerably speeded up the importing of files from other software. e.g. a MOSS file which used to take over  3 minutes to get in now takes around 30 seconds.





Export DWG – symbols from CDS are now exported as Blocks in Autocad.





Contouring – if you had a very long job name, (over 50 characters) CDS may have refused to contour correctly. This has been rectified.





Zoom Previous and Zoom magnification have now been re-instated.





Heights were previously displayed and plotted to 2 decimal paces regardless of what you did. – now fixed.





Points – Select Range – had problems if NULL was involved – now fixed.





Cogo – Road Calcs – Truncations (the old Splays) has been added


Cogo – Road Calcs – Autoroad will now store calculated chainages and offsets if a Road Number has been set.


Cogo – Road Calcs  - Autoroad – will now allow you to specify a height correction for each offset if required.


Cogo – Road Calcs - Parallel had problems with the half angle on some jobs, and, would not work if you had a series of lines along the same straight – both misdemeanours corrected.





Cogo – Stakeout – you can now specify a series of Setup stations for the Radial report.





Cogo – 2 Distance Intersection – was putting the calculated points on Layer 0 regarless of what you had set as the current layer – now re-educated.





Version 1.03 Release April 23 1999





Any changes contained in this release have been documented in the Release Notes shipped with this CD or Disk set.





The On Line manual has also been updated to reflect the changes in this release.





Any things which have been noticed after the release notes and on-line manual were completed are contained in this file.





Please read through and NOTE the following items:





Symbols





Previous versions of CDS used Windows Metafiles. They use an extension of "WMF". This version will use any existing symbols; but has the ability to use enhanced metafiles "EMF". Enhanced metafiles are recommended but you can still create new symbols in an WMF format if you wish.


The enhanced metafile has the advantage that it knows internally at what size it was created. The symbol library in CDS can use this when first registering the symbol. You can however overwrite this size if you wish; but remember that rereading the symbol library will overwrite this size with the creation size of  the metafile.


If you wish to retain the pre-existing symbols and sizes; and don't want to install any new ones then do a custom installation making sure that you tick everything except the locked files.


If you browse the release CD you may notice a folder called "RTA symbols". If you want to use these symbols then copy them as well to the "Foresite\variable" folder. You will have to reread the symbol library.


All the symbols supplied as default with CDS have been created at a nominal scale of 5mm.  If you want a different size you have two main options. You can change the magnification factor in any code library's you use. This is the preferred option. Alternatively you can redo the metafile. A shareware program called metafile companion has been included on the release CD. This allows you to edit existing metafiles or create your own. There are other programs around if you so desire.





Use of Metafile Companion


This is a shareware program. To install it run the setup program from the MetafileCompanion folder on the release CD. It allows you a number of free goes. After that you need to register for about $30 US. There is online help program.








Profiles & Sections


If you load an old Road job into this version, you may need to redo your Profile & Section parameters.





If your Section is displayed with a thick line, you should access section plotting parameters, and then select the Linetype tab for the relevant sections. Change the 'Width' back to 1 and when you return to the display all will be well





Running under Windows NT	





Windows NT is the preferred environment for CDS due to it's more robust nature. An additional driver for the hardware dongle needs to be installed however; as NT does not allow the program to access the parallel port directly. Note you only have to install this driver once. If your program already runs under NT nothing needs to be done; as it has already been installed. The setup program can be found in the NTDisk folder on the CDS CD. For additional information and further utility checking programs you are best accessing the rainbow web site directly. It can be found at WWW.RNBO.COM








A note about Hardware Locks/Dongles





Please note that if you do not have a valid dongle installed in one of


your Printer ports when you start the program, it will operate in "Demo" mode.


This will allow you to process a limited part of your job, but all options 


concerned with export or printing/plotting will be disabled.





Also various design options which are not part of TRPS will be disabled.





If you have a TRPS dongle DO NOT plug a Zip drive into it - it is almost certain


to damage the lock, and we will not carry the cost of any locks damaged in this fashion.


You should plug the Zip directly into the computer, and then, if you must, 


put the dongle into the back of the Zip drive, and then plug the 


Printer cord into the dongle.





The CDS dongles do not seem to have the same sensitivity to Zip drives, but for safety


we recommend that you plug them into the Zip drive rather than the computer. 








