                     Calculation of Volumes Between Surfaces

Date:  31/10/2017

VOLUME CALCULATION = TOPO vs EGL (27/10/17)
Base Job   : G:\3A JBD FILES\DATA\DWG FILES\ERNA\2017\VOLUME KOLAM\topo.cdsdat       Surface: Surface1 (Natural)

Overlay Job: G:\3A JBD FILES\DATA\DWG FILES\ERNA\2017\VOLUME KOLAM\0PondA_Resurvey\0PondA_Resurvey\egl_171031.cdsdat       Surface: Surface1 (Natural)

Fill Surface Area : 32855.019 sq. metres

Fill Area: 32416.394 sq. metres  Fill Volume : 30688.878 cubic metres

Cut Surface Area : 136517.937 sq. metres

Cut Area: 117060.306 sq. metres  Cut Volume : -281251.663 cubic metres

Matching Surface Area :    0.368 sq. metres

Matching Area         :    0.368 sq. metres
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