1 piles positons,  pilecaps centre and sizes 
 				- RM4 @ PER PILE 
 				- RM6 @ PER PILECAP 
   				- RM 6 @ STARTER BAR
2. ground beams positions and sizes	
 				 - RM 5 @ GROUND BEAMS (PER SEGMENT, between column to column)
3 footprint of ground floor slabs with levels at 10m intervals
                                                        -  Lump Sump – (Depend on site situation, need to site Visit)
4 column positions and lift cores postions at ground floor including verticality check at XY postions and sizes		 		- RM 5 PER COLUMN (As-built 3 pts per column)
				- RM 100 PER LIFT CORE (As-built Inside the wall for every single lift core)
5.1st floor beams postions and sizes		
				- RM 7 @  BEAMS (PER SEGMENT, between column to column)	
6 Footprint of 1st floor slabs and levels at 10m intervals
  			-  Lump Sump – (Depend on site situation, need to site Visit)
7. 1st floor column positions, lift ore postions and sizes
- RM 5 PER COLUMN (As-built 3 pts per column)
				- RM 100 PER LIFT CORE (As-built Inside the wall for every single lift core)
8 External walls, ramps, staircase and road positions
				- RM 6 @  Wall (PER SEGMENT, between column to column)
- RM 50 @  Staircase  (4 pts per staircase)
- Road position -Lump Sump – (Depend on site situation, need to site Visit)
[bookmark: _GoBack]9 Sumps and drains positions and sizes
 			- Lump Sump – (Depend on site situation, need to site Visit)

10. Daywork rates  (time from starting to ending for the day)- for additonal works
- Daywork RM500 + additional RM250 (Outstation) per trip (7.00a.m. to 1p.m.)
