FOO CHEE YONG
No 21, Jalan Putra Permai 10/2J, Putra Heights 47650 Subang Jaya, Selangor.

H/P : 012-281 9844

Our Ref     : GTS/TTW/Q2511


        

          14th March2021
TT WATER SDN. BHD.
(Water Dept. Project Office)

No. 11-1, Jalan 11/62A, 

Bandar Menjalara, Kepong, 

52200, Kuala Lumpur, 

Wilayah Persekutuan Kuala Lumpur, 

Malaysia

Tel. : 603 6274 0888

Fax :  603 6274 1888 
Email : slyam@tenagatiub.com.my
Dear Mr. Yam,
CADANGAN KERJA-KERJA PEMBEKALAN, PEMASANGAN, PENGUJIAN DAN PENTAULIAHAN SISTEM PENGEPAMAN ARCHIMEDEAN PUMP DAN KERJA KERJA LAIN BERKIATAN DI KOLAM HORAS 600 KAMPUNG SG. DARAH, BESTARI JAYA, KUALA SELANGOR, SELANGOR DARUL .
With reference to the above, we are pleased to submit herewith our quotation for your kind approval.

	No
	Type of work
	Amount (RM)

	1.
2.

3.

4.
5.


	Prepare control points and existing main feature Checking to local boundary stone.

Transfer TBM with based on government bench mark.

Topo Survey On Related area. (Lump Sum)

Setting Out Survey For Main structure. (Lump Sum)
Plotting & Produced Survey plan on suitable scale.

Licensed Surveyor Endorsed plan on as-built drawing. 

	RM1000.00
RM500.00
RM2000.00

RM2000.00
RM500.00 

RM500.00

	
	
	

	
	Total
	RM6500.00


Note:
Any re-peg for missing, distrusted points will have additional charges.
Any Additional trip will be charges with RM500 per trips.   
Schedule of Payment: Survey fees should be paid by stages upon complete of the item of survey works. 
We trust the above will meet your kind requirements. Should you need any further detail, please do not hesitate to contact us.

Thank you.

Yours faithfully,

Foo Chee Yong.

Client’s Acceptance

I / we, hereby agreed to accept your offer for the abovementioned services as per your letter GTS/TTW/Q2511
 dated 14th March2021 subject to the term and conditions of the contents therein.

……………………………….                

         …………………………….

               (Signature)






(Witness)

Name: …………………




Name:…………………

Date  : …………………




Date  : …………..……..

Company Stamp: …………………………….

