VOLUME CALCULATION = OGL vs EGL

                              Foresight Software Pty Ltd

                     Calculation of Volumes Between Surfaces

Date:  12/05/2014

Base Job   : J:\3JBD FILES\DWG FILES\ERNA\Foo164_Sg_Kerayong\Foo164_Sg_Kerayong\db.ogl       Surface: Surface1 (Natural)

Overlay Job: J:\3JBD FILES\DWG FILES\ERNA\Foo164_Sg_Kerayong\Foo164_Sg_Kerayong\db.egl       Surface: Surface1 (Natural)

Fill Surface Area :    0.000 sq. metres

Fill Area:    0.000 sq. metres  Fill Volume :    0.000 cubic metres

Cut Surface Area : 10765.270 sq. metres

Cut Area: 10764.314 sq. metres  Cut Volume : -16436.777 cubic metres

Matching Surface Area :    0.000 sq. metres

Matching Area         :    0.000 sq. metres

