Property Report 12/2/2023
Keys
8 Jan 2023
Alex had handed over the property file and 1 set of church van key, sanctuary door key and staircase key to fFo.
11 Jan 2023
Done duplicating of the 3rd set property’s keys (Church Van, Sanctuary Door & Staircase).
Key Keeper: Pastor Lee, Alex Lim, Foo Chee Yong.

Trimming Tree Activity
7 Jan 2023 
Trim 3 trees near the main gate church.

11 Feb 2023
Trim 4 trees below transmission line on the left side of church.

Repair Work
8 Jan 2023
Install 2 units of hanger at new pantry

15 Jan 2023
Church member was complained on water did not flow on female toilet bowl. Repaired work already done by new building’s contractor. 

18 Jan 2023
Repair the staircase door lock pad.

05 Feb 2023
Church member was complained about leaking on male toilet bowl. Repaired work already done by new building’s contractor. 





Sanctuary Leaking 
Leakage points 1
Location: Top glass panel (between panel 1 and 2) on top of stage,
Reason: old ages of sealant on the glass and aluminum frame.
Solution : Replace the sealant with waterproof tape.
Status: Repaired and no more leakage.

Leakage points 2
Location: top glass panel on top of 1st floor seating area,
Reason: old ages of sealant on glass, aluminum frame & concreate wall
Solution : Replace the sealant and adding with waterproof tape.
Status: Water proof sealant replaced and waiting for adding the waterproof tape (Still under observation for leakage).

Leakage points 3
Location: Top of Wall (left wall sanctuary)
Reason: We found that the original roof caping is too small and not fully cover the beam.
Solution : We already do some repairing and still need some improvement on that area. Scarf folding still install on that area to observe the leakage area. 
Status : Repair works in progress

Leakage points 4
Location: top glass panel (panel 4) on top of stage,
Reason: old ages of sealant on glass and aluminum frame.
Solution : Replace the sealant with waterproof tape.
Status: New leaking spot and waiting to replace the sealant and waterproof tape

Leakage points 5
Location: Font left steel door,
Reason: Design and structure failure. 
Solution : Suggest to add some rubber or steel plate on top of the door to avoid rain water come in
Status: Preparation



Leakage points 6
Location: Behind left steel door,
Reason: Design and structure failure. 
Solution : Suggest to add some rubber or steel plate on top of the door to avoid rain water come in
Status: preparation

    
